#*******************************************************************
#
# $Source: /sc/CvsTree/sc/gen/src/form/ased_acqu.form,v $
#
# Copyright (c) 1995 - 2008
# BRUKER BioSpin GmbH
# D-76287 Rheinstetten, Germany
#
# All Rights Reserved
#
#
# $Id: ased_acqu.form,v 1.18.2.1 2011/02/25 13:20:57 es Exp $
#*******************************************************************
EDIT_PAR COMMAND FILE

DI_MODE         LONG
ED_ENTRY        ACQU
ORDER           FILE


HEADER		"====== General ======"
NAME		PULPROG
END
NAME		TD
END
NAME		SW
END
T_NAME		SWH
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"SWH=SW*SFO1"
		INV_REL "SW=SWH/SFO1"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"sweep width"
END
T_NAME          AQ
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"AQ=aqcalc(SW,SFO1,TD,DIGTYP)"
		INV_REL	"TD=tdcalc(SW,SFO1,1.0e6*AQ,DIGTYP)"
		UNIT	"sec"
		FORMAT	"%14.7f sec"
                TEXT	"acquisition time"
END
NAME		RG
END
T_NAME          DW
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"DW=1/(2*SW*SFO1)"
		INV_REL	"SW=1000000/(2*(0.005+DW)*SFO1)"
		UNIT	"usec"
		FORMAT	"%14.3f usec"
		TEXT	"dwell time "
END
NAME		DE
		FORMAT	"%14.2f usec"
END
T_NAME		CNST2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"CNST2=CNST[2]"
		INV_REL	"CNST[2]=CNST2"
		FORMAT	"%14.7f"
		TEXT		"> J(HH); 30 Hz"
END
T_NAME		d0
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d0=in0/2"
		INV_REL	"D[0]=d0"
		UNIT	"sec"
		TEXT		"incremented delay (2D)                           [3 usec]"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		D1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D1=D[1]"
		INV_REL	"D[1]=D1"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT		"relaxation delay; 1-5 * T1"
END
T_NAME		d4
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d4=1s/(cnst2*4)"
		INV_REL	"D[0]=d4"
		UNIT	"sec"
		TEXT		"1/(4J(HH))"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d11
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d11=30m"
		INV_REL	"D[0]=d11"
		UNIT	"sec"
		TEXT		"delay for disk I/O                               [30 msec]"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		D16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D16=D[16]"
		INV_REL	"D[16]=D16"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT		"delay for homospoil/gradient recovery"
END
NAME		DS
		TEXT	"number of dummy scans"
END
T_NAME		in0
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"in0=inf1"
		INV_REL	"D[0]=in0"
		UNIT	"sec"
		TEXT		"1/(2 * SW(X)) = DW(X)"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		INF1
		TYPE	R64
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"INF1=INF[1]"
		INV_REL	"INF[1]=INF1"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT		"1/SW(X) = 2 * DW(X)"
		NONEDIT
END
NAME		NS
		TEXT	"scans to execute"
END
HEADER		"======== CHANNEL f1 ========"
NAME		SFO1
		FORMAT	"%14.7f MHz"
		TEXT	"frequency of ch. 1"
END
NAME		O1
		FORMAT	"%14.2f Hz"
		TEXT	"frequency of ch. 1"
END
T_NAME		O1P
		TYPE	R64
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"O1P=O1/BF1"
		INV_REL	"O1=O1P*BF1"
		UNIT	"ppm"
		FORMAT	"%14.3f ppm"
		TEXT	"frequency of ch. 1"
END
NAME		NUC1
		NONEDIT
		TEXT	"nucleus for channel 1"
END
T_NAME		P13
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P13=P[13]"
		INV_REL	"P[13]=P13"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT		"550u"
END
T_NAME		P14
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P14=P[14]"
		INV_REL	"P[14]=P14"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT		"200u"
END
T_NAME		P15
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P15=P[15]"
		INV_REL	"P[15]=P15"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT		"200u"
END
T_NAME		P23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P23=P[23]"
		INV_REL	"P[23]=P23"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT		"1st inversion pulse for dephasing (z-filter)"
END
T_NAME		P24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P24=P[24]"
		INV_REL	"P[24]=P24"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT		"2nd inversion pulse for dephasing (z-filter)"
END
T_NAME		PLW0
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 100
		REL	"PLW0=PLW[0]"
		INV_REL	"PLW[0]=PLW0"
		UNIT	"W"
		FORMAT	"%14.5g W"
		TEXT		"0W"
END
T_NAME		PLdB0
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -20.1 1000
		REL	"if(PLW[0]>0)PLdB0=-10*log(PLW[0])/LN10;else PLdB0=1000;"
		INV_REL	"PLW[0]=0;if(PLdB0<1000)PLW[0]=pow(10.0,(-PLdB0)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f -dBW"
		TEXT	"power PL0 in -dBW"
END
T_NAME		PLW1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 100
		REL	"PLW1=PLW[1]"
		INV_REL	"PLW[1]=PLW1"
		UNIT	"W"
		FORMAT	"%14.5g W"
		TEXT		"power level for pulse (default)"
END
T_NAME		PLdB1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -20.1 1000
		REL	"if(PLW[1]>0)PLdB1=-10*log(PLW[1])/LN10;else PLdB1=1000;"
		INV_REL	"PLW[1]=0;if(PLdB1<1000)PLW[1]=pow(10.0,(-PLdB1)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f -dBW"
		TEXT	"power PL1 in -dBW"
END
NAME		SPNAM[13]
		TEXT		"jc08_BEBOP_z-y_550u_BW10..."
END
T_NAME		SPOAL13
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL13=SPOAL[13]"
		INV_REL	"SPOAL[13]=SPOAL13"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP13"
END
T_NAME		SPOFFS13
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS13=SPOFFS[13]"
		INV_REL	"SPOFFS[13]=SPOFFS13"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP13"
END
T_NAME		SPW13
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 100
		REL	"SPW13=SPW[13]"
		INV_REL	"SPW[13]=SPW13"
		UNIT	"W"
		FORMAT	"%14.5g W"
		TEXT		"20 kHz: Power level for 12.5us 90° pulse"
END
T_NAME		SPdB13
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -20.1 1000
		REL	"if(SPW[13]>0)SPdB13=-10*log(SPW[13])/LN10;elseSPdB13=1000;"
		INV_REL	"SPW[13]=0;if(SPdB13<1000)SPW[13]=pow(10.0,(-SPdB13)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f -dBW"
		TEXT	"power SPW13 in -dBW"
END
NAME		SPNAM[14]
		TEXT		"URx180_200_0.5u_BW10..."
END
T_NAME		SPOAL14
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL14=SPOAL[14]"
		INV_REL	"SPOAL[14]=SPOAL14"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP14"
END
T_NAME		SPOFFS14
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS14=SPOFFS[14]"
		INV_REL	"SPOFFS[14]=SPOFFS14"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP14"
END
T_NAME		SPW14
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 100
		REL	"SPW14=SPW[14]"
		INV_REL	"SPW[14]=SPW14"
		UNIT	"W"
		FORMAT	"%14.5g W"
		TEXT		"20 kHz: Power level for 12.5us 90° pulse"
END
T_NAME		SPdB14
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -20.1 1000
		REL	"if(SPW[14]>0)SPdB14=-10*log(SPW[14])/LN10;elseSPdB14=1000;"
		INV_REL	"SPW[14]=0;if(SPdB14<1000)SPW[14]=pow(10.0,(-SPdB14)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f -dBW"
		TEXT	"power SPW14 in -dBW"
END
NAME		SPNAM[15]
		TEXT		"jc20_BURBOP_x90.0deg..."
END
T_NAME		SPOAL15
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL15=SPOAL[15]"
		INV_REL	"SPOAL[15]=SPOAL15"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP15"
END
T_NAME		SPOFFS15
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS15=SPOFFS[15]"
		INV_REL	"SPOFFS[15]=SPOFFS15"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP15"
END
T_NAME		SPW15
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 100
		REL	"SPW15=SPW[15]"
		INV_REL	"SPW[15]=SPW15"
		UNIT	"W"
		FORMAT	"%14.5g W"
		TEXT		"20 kHz: Power level for 12.5us 90° pulse"
END
T_NAME		SPdB15
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -20.1 1000
		REL	"if(SPW[15]>0)SPdB15=-10*log(SPW[15])/LN10;elseSPdB15=1000;"
		INV_REL	"SPW[15]=0;if(SPdB15<1000)SPW[15]=pow(10.0,(-SPdB15)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f -dBW"
		TEXT	"power SPW15 in -dBW"
END
NAME		SPNAM[16]
		TEXT		"jc04_BEBOP_yz_550u..."
END
T_NAME		SPOAL16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL16=SPOAL[16]"
		INV_REL	"SPOAL[16]=SPOAL16"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP16"
END
T_NAME		SPOFFS16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS16=SPOFFS[16]"
		INV_REL	"SPOFFS[16]=SPOFFS16"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP16"
END
T_NAME		SPW16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 100
		REL	"SPW16=SPW[16]"
		INV_REL	"SPW[16]=SPW16"
		UNIT	"W"
		FORMAT	"%14.5g W"
		TEXT		"20 kHz: Power level for 12.5us 90° pulse"
END
T_NAME		SPdB16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -20.1 1000
		REL	"if(SPW[16]>0)SPdB16=-10*log(SPW[16])/LN10;elseSPdB16=1000;"
		INV_REL	"SPW[16]=0;if(SPdB16<1000)SPW[16]=pow(10.0,(-SPdB16)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f -dBW"
		TEXT	"power SPW16 in -dBW"
END
NAME		SPNAM[23]
		TEXT		"1st inversion pulse for dephasing (z-filter)"
END
T_NAME		SPOAL23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL23=SPOAL[23]"
		INV_REL	"SPOAL[23]=SPOAL23"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP23"
END
T_NAME		SPOFFS23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS23=SPOFFS[23]"
		INV_REL	"SPOFFS[23]=SPOFFS23"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP23"
END
T_NAME		SPW23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 100
		REL	"SPW23=SPW[23]"
		INV_REL	"SPW[23]=SPW23"
		UNIT	"W"
		FORMAT	"%14.5g W"
		TEXT		"Power level for dephasing pulse (z-filter)"
END
T_NAME		SPdB23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -20.1 1000
		REL	"if(SPW[23]>0)SPdB23=-10*log(SPW[23])/LN10;elseSPdB23=1000;"
		INV_REL	"SPW[23]=0;if(SPdB23<1000)SPW[23]=pow(10.0,(-SPdB23)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f -dBW"
		TEXT	"power SPW23 in -dBW"
END
NAME		SPNAM[24]
		TEXT		"2nd inversion pulse for dephasing (z-filter)"
END
T_NAME		SPOAL24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL24=SPOAL[24]"
		INV_REL	"SPOAL[24]=SPOAL24"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP24"
END
T_NAME		SPOFFS24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS24=SPOFFS[24]"
		INV_REL	"SPOFFS[24]=SPOFFS24"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP24"
END
T_NAME		SPW24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 100
		REL	"SPW24=SPW[24]"
		INV_REL	"SPW[24]=SPW24"
		UNIT	"W"
		FORMAT	"%14.5g W"
		TEXT		"Power level for dephasing pulse (z-filter)"
END
T_NAME		SPdB24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -20.1 1000
		REL	"if(SPW[24]>0)SPdB24=-10*log(SPW[24])/LN10;elseSPdB24=1000;"
		INV_REL	"SPW[24]=0;if(SPdB24<1000)SPW[24]=pow(10.0,(-SPdB24)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f -dBW"
		TEXT	"power SPW24 in -dBW"
END
HEADER		"====== GRADIENT CHANNEL ====="
NAME		GPNAM[3]
		TEXT		"SMSQ10.100"
END
T_NAME		GPZ1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ1=GPZ[1]"
		INV_REL	"GPZ[1]=GPZ1"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT		"7.2% z-filter gradient"
END
T_NAME		GPZ2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ2=GPZ[2]"
		INV_REL	"GPZ[2]=GPZ2"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT		"-7.5% z-filter gradient"
END
T_NAME		GPZ3
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ3=GPZ[3]"
		INV_REL	"GPZ[3]=GPZ3"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT		"-17.9% purge gradient"
END
T_NAME		P16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P16=P[16]"
		INV_REL	"P[16]=P16"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT		"homospoil/gradient pulse                         [1 msec]"
END
