CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.1/conf/instr/spect/uxnmr.info
Date         : Fri Feb 28 18:11:35 2014
Release      : TopSpin Acquisition Version 3.1-pl6
Installed in : C:/Bruker/TopSpin3.1
Host         : INT-PAULI
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 2533 MHz)
User         : nmr
Description  : Avance II
Location     : Karlsruher Institut fuer Technologie
System       : Avance-AV NMR spectrometer
1H-frequency : 600.19 MHz
Order Number : 10072783
Configured in: C:/Bruker/TopSpin3.1/conf/instr/spect

#--------------------
#  FCU configuration:
#--------------------
board # 1 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 2 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 3 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 4 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)

DRU: AQS DRU-E Z102520/00053 ECL 00.01
- TCP/IP address = 149.236.99.89
- Firmware Version = 130419

Gcu: GCU3_SlowIF

AQS: connected to spect:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x62   0x3    AV  R  4.0 REC-1  AQS RXAD-BB Z102119/50 ECL 04.00
     3   0x34 0xc0   0x1        X  0.4 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x18   0x4    BH  S  2.1 SGU-1  AQS SGU600 Z003831/01670 ECL 2.1
     5   0x25 0x18   0x4    BH  S  2.1 SGU-2  AQS SGU600 Z003831/01674 ECL 2.1
     6   0x26 0x18   0x4    BH  S  1.1 SGU-3  AQS SGU600 Z003831/01205 ECL 1.1
     9   0x3c  0x4     0        Y  1.0 ROUT-1 Avance Router 3/5
    21   0x21  0xa     0        P  1.0 PSD-1  Power Supply Distribution Board
    25   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 Avance-Router

Amplifier Control Board:  connected to spect:/dev/tty20


Amplifiers (ACB configuration):
  RO  Amplifier  Module  Nucleus  Power/W  Switchbox Name PN/SN/FW
   1      1         1        X      300    N  (V=ff) BLAXH2H 300/100/150 W1345080/59/20071205
   2      1         2       1H      100    N  (-""-) BLAXH2H 300/100/150 W1345080/59/20071205
   3      1         3       2H      150    N         BLAXH2H 300/100/150 W1345080/59/20071205



- Type: BSMS/1
- absolute lockshift frequency =  12132819 Hz
- GAB type = GAB
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)

Bruker Automatic Changer: device connected to spect:/dev/tty04
- Capacity: 120 holders
- Firmware: 20040805
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

Lock: device connected to spect:/dev/tty03

MAS2 control unit: connected to spect:/dev/tty07
MAS2: device not yet configured
MAS1: device could not be configured

Eurotherm VTU: device connected to spect:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to spect:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                 PN=Z003462, SN=00497 from 20070103
    Module  2 : 2H
                 PN=Z003473, SN=00498 from 20070108
    Module  3 : XBB19F 2HS
                 PN=Z003506, SN=00544 from 20070105


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU



