#*******************************************************************
#
# $Source: /sc/CvsTree/sc/gen/src/form/ased_acqu.form,v $
#
# Copyright (c) 1995 - 2008
# BRUKER BioSpin GmbH
# D-76287 Rheinstetten, Germany
#
# All Rights Reserved
#
#
# $Id: ased_acqu.form,v 1.16.2.1 2009/11/27 16:29:43 ge Exp $
#*******************************************************************
EDIT_PAR COMMAND FILE

DI_MODE         LONG
ED_ENTRY        ACQU
ORDER           FILE


HEADER		"====== General ======"
NAME		PULPROG
END
NAME		TD
END
NAME		SW
END
T_NAME		SWH
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"SWH=SW*SFO1"
		INV_REL "SW=SWH/SFO1"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"sweep width"
END
T_NAME          AQ
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"AQ=aqcalc(SW,SFO1,TD,DIGTYP)"
		INV_REL	"TD=tdcalc(SW,SFO1,1.0e6*AQ,DIGTYP)"
		UNIT	"sec"
		FORMAT	"%14.7f sec"
                TEXT	"acquisition time"
END
NAME		RG
END
T_NAME          DW
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"DW=1/(2*SW*SFO1)"
		INV_REL	"SW=1000000/(2*(0.005+DW)*SFO1)"
		UNIT	"usec"
		FORMAT	"%14.3f usec"
		TEXT	"dwell time "
END
NAME		DE
		FORMAT	"%14.2f usec"
END
T_NAME		d0
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d0=3u"
		INV_REL	"D[0]=d0"
		UNIT	"sec"
		TEXT	"d0=3u"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		D1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D1=D[1]"
		INV_REL	"D[1]=D1"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
TEXT		"relaxation delay; 1-5 * T1"
END
T_NAME		D5
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D5=D[5]"
		INV_REL	"D[5]=D5"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
TEXT		"= 1 (for J=120-250Hz, Delay Scaling Factor)"
END
T_NAME		d11
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d11=30m"
		INV_REL	"D[0]=d11"
		UNIT	"sec"
		TEXT	"d11=30m"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		D16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D16=D[16]"
		INV_REL	"D[16]=D16"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
TEXT		"delay for homospoil/gradient recovery"
END
T_NAME		d20
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d20=d5*0.001469"
		INV_REL	"D[0]=d20"
		UNIT	"sec"
		TEXT	"d20=d5*0.001469"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d21
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d21=d5*0.00213465"
		INV_REL	"D[0]=d21"
		UNIT	"sec"
		TEXT	"d21=d5*0.00213465"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d22
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d22=d5*0.0003938"
		INV_REL	"D[0]=d22"
		UNIT	"sec"
		TEXT	"d22=d5*0.0003938"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		DELTA
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"DELTA=p16+d16+p26+d0*2"
		INV_REL	"D[0]=DELTA"
		UNIT	"sec"
		TEXT	"DELTA=p16+d16+p26+d0*2"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		DELTA1
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"DELTA1=d5*0.001469-p16-4u"
		INV_REL	"D[0]=DELTA1"
		UNIT	"sec"
		TEXT	"DELTA1=d5*0.001469-p16-4u"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		DELTA3
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"DELTA3=p16+d16-4u"
		INV_REL	"D[0]=DELTA3"
		UNIT	"sec"
		TEXT	"DELTA3=p16+d16-4u"
		FORMAT	"%14.8f sec"
		NONEDIT
END
NAME		DS
		TEXT	"number of dummy scans"
END
T_NAME		in0
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"in0=inf1/2"
		INV_REL	"D[0]=in0"
		UNIT	"sec"
		TEXT	"in0=inf1/2"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		INF1
		TYPE	R64
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"INF1=INF[1]"
		INV_REL	"INF[1]=INF1"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"1/SW(X) = 2 * DW(X)"
		NONEDIT
END
NAME		NS
		TEXT	"scans to execute"
END
T_NAME		P1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P1=P[1]"
		INV_REL	"P[1]=P1"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"f1 channel -  90 degree high power pulse"
END
T_NAME		p2
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"p2=p1*2"
		INV_REL	"D[0]=p2"
		UNIT	"usec"
		TEXT	"p2=p1*2"
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		P3
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P3=P[3]"
		INV_REL	"P[3]=P3"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"f2 channel -  90 degree high power pulse"
END
T_NAME		p4
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"p4=p3*2"
		INV_REL	"D[0]=p4"
		UNIT	"usec"
		TEXT	"p4=p3*2"
		FORMAT	"%14.2f usec"
		NONEDIT
END
HEADER		"======== CHANNEL f1 ========"
NAME		NUC1
		NONEDIT
		TEXT	"nucleus for channel 1"
END
NAME		O1
		FORMAT	"%14.2f Hz"
		TEXT	"frequency of ch. 1"
END
T_NAME		O1P
		TYPE	R64
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"O1P=O1/BF1"
		INV_REL	"O1=O1P*BF1"
		UNIT	"ppm"
		FORMAT	"%14.3f ppm"
		TEXT	"frequency of ch. 1"
END
T_NAME		P21
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P21=P[21]"
		INV_REL	"P[21]=P21"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"550u excitation pulses"
END
T_NAME		P22
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P22=P[22]"
		INV_REL	"P[22]=P22"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"600u UR and Inversion pulses"
END
T_NAME		P26
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P26=P[26]"
		INV_REL	"P[26]=P26"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"100u Inversion pulse"
END
T_NAME		P30
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P30=P[30]"
		INV_REL	"P[30]=P30"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"200u odd UR pulses"
END
T_NAME		PLW1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"PLW1=PLW[1]"
		INV_REL	"PLW[1]=PLW1"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"f1 channel - power level for pulse (default)"
END
T_NAME		PLdB1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -19.4574 1000
		REL	"if(PLW[1]>0)PLdB1=-10*log(PLW[1])/LN10;else PLdB1=1000;"
		INV_REL	"PLW[1]=0;if(PLdB1<1000)PLW[1]=pow(10.0,(-PLdB1)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power PL1 in dB"
END
NAME		SFO1
		FORMAT	"%14.7f MHz"
		TEXT	"frequency of ch. 1"
END
NAME		SPNAM21
TEXT		"jc01_BEBOP_zx.."
END
T_NAME		SPOAL21
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL21=SPOAL[21]"
		INV_REL	"SPOAL[21]=SPOAL21"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP21"
END
T_NAME		SPOFFS21
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS21=SPOFFS[21]"
		INV_REL	"SPOFFS[21]=SPOFFS21"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP21"
END
T_NAME		SPW21
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW21=SPW[21]"
		INV_REL	"SPW[21]=SPW21"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"20 kHz Rf Amplitude"
END
T_NAME		SPdB21
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -19.4574 1000
		REL	"if(SPW[21]>0)SPdB21=-10*log(SPW[21])/LN10;elseSPdB21=1000;"
		INV_REL	"SPW[21]=0;if(SPdB21<1000)SPW[21]=pow(10.0,(-SPdB21)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power SPW21 in dB"
END
NAME		SPNAM22
TEXT		"jc02_BURBOP_x.."
END
T_NAME		SPOAL22
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL22=SPOAL[22]"
		INV_REL	"SPOAL[22]=SPOAL22"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP22"
END
T_NAME		SPOFFS22
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS22=SPOFFS[22]"
		INV_REL	"SPOFFS[22]=SPOFFS22"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP22"
END
T_NAME		SPW22
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW22=SPW[22]"
		INV_REL	"SPW[22]=SPW22"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"20 kHz Rf Amplitude"
END
T_NAME		SPdB22
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -19.4574 1000
		REL	"if(SPW[22]>0)SPdB22=-10*log(SPW[22])/LN10;elseSPdB22=1000;"
		INV_REL	"SPW[22]=0;if(SPdB22<1000)SPW[22]=pow(10.0,(-SPdB22)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power SPW22 in dB"
END
NAME		SPNAM24
TEXT		"jc04_BEBOP_yz.."
END
T_NAME		SPOAL24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL24=SPOAL[24]"
		INV_REL	"SPOAL[24]=SPOAL24"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP24"
END
T_NAME		SPOFFS24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS24=SPOFFS[24]"
		INV_REL	"SPOFFS[24]=SPOFFS24"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP24"
END
T_NAME		SPW24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW24=SPW[24]"
		INV_REL	"SPW[24]=SPW24"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"20 kHz Rf Amplitude"
END
T_NAME		SPdB24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -19.4574 1000
		REL	"if(SPW[24]>0)SPdB24=-10*log(SPW[24])/LN10;elseSPdB24=1000;"
		INV_REL	"SPW[24]=0;if(SPdB24<1000)SPW[24]=pow(10.0,(-SPdB24)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power SPW24 in dB"
END
NAME		SPNAM26
TEXT		"jc06_BIBOP_z-z.."
END
T_NAME		SPOAL26
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL26=SPOAL[26]"
		INV_REL	"SPOAL[26]=SPOAL26"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP26"
END
T_NAME		SPOFFS26
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS26=SPOFFS[26]"
		INV_REL	"SPOFFS[26]=SPOFFS26"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP26"
END
T_NAME		SPW26
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW26=SPW[26]"
		INV_REL	"SPW[26]=SPW26"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"20 kHz Rf Amplitude"
END
T_NAME		SPdB26
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -19.4574 1000
		REL	"if(SPW[26]>0)SPdB26=-10*log(SPW[26])/LN10;elseSPdB26=1000;"
		INV_REL	"SPW[26]=0;if(SPdB26<1000)SPW[26]=pow(10.0,(-SPdB26)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power SPW26 in dB"
END
NAME		SPNAM28
TEXT		"jc08_BEBOP_z-y.."
END
T_NAME		SPOAL28
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL28=SPOAL[28]"
		INV_REL	"SPOAL[28]=SPOAL28"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP28"
END
T_NAME		SPOFFS28
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS28=SPOFFS[28]"
		INV_REL	"SPOFFS[28]=SPOFFS28"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP28"
END
T_NAME		SPW28
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW28=SPW[28]"
		INV_REL	"SPW[28]=SPW28"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"20 kHz Rf Amplitude"
END
T_NAME		SPdB28
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -19.4574 1000
		REL	"if(SPW[28]>0)SPdB28=-10*log(SPW[28])/LN10;elseSPdB28=1000;"
		INV_REL	"SPW[28]=0;if(SPdB28<1000)SPW[28]=pow(10.0,(-SPdB28)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power SPW28 in dB"
END
NAME		SPNAM30
TEXT		"jc10_BURBOP_x242.8833deg.."
END
T_NAME		SPOAL30
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL30=SPOAL[30]"
		INV_REL	"SPOAL[30]=SPOAL30"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP30"
END
T_NAME		SPOFFS30
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS30=SPOFFS[30]"
		INV_REL	"SPOFFS[30]=SPOFFS30"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP30"
END
T_NAME		SPW30
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW30=SPW[30]"
		INV_REL	"SPW[30]=SPW30"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"20 kHz Rf Amplitude"
END
T_NAME		SPdB30
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -19.4574 1000
		REL	"if(SPW[30]>0)SPdB30=-10*log(SPW[30])/LN10;elseSPdB30=1000;"
		INV_REL	"SPW[30]=0;if(SPdB30<1000)SPW[30]=pow(10.0,(-SPdB30)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power SPW30 in dB"
END
NAME		SPNAM31
TEXT		"jc11_BURBOP_x65.3166deg.."
END
T_NAME		SPOAL31
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL31=SPOAL[31]"
		INV_REL	"SPOAL[31]=SPOAL31"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP31"
END
T_NAME		SPOFFS31
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS31=SPOFFS[31]"
		INV_REL	"SPOFFS[31]=SPOFFS31"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP31"
END
T_NAME		SPW31
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW31=SPW[31]"
		INV_REL	"SPW[31]=SPW31"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"20 kHz Rf Amplitude"
END
T_NAME		SPdB31
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -19.4574 1000
		REL	"if(SPW[31]>0)SPdB31=-10*log(SPW[31])/LN10;elseSPdB31=1000;"
		INV_REL	"SPW[31]=0;if(SPdB31<1000)SPW[31]=pow(10.0,(-SPdB31)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power SPW31 in dB"
END
HEADER		"======== CHANNEL f2 ========"
NAME		NUC2
		NONEDIT
		TEXT	"nucleus for channel 2"
END
NAME		O2
		FORMAT	"%14.2f Hz"
		TEXT	"frequency of ch. 2"
END
T_NAME		O2P
		TYPE	R64
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"O2P=O2/BF2"
		INV_REL	"O2=O2P*BF2"
		UNIT	"ppm"
		FORMAT	"%14.3f ppm"
		TEXT	"frequency of ch. 2"
END
T_NAME		P27
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P27=P[27]"
		INV_REL	"P[27]=P27"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"1100u UR pulse"
END
T_NAME		PLW2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"PLW2=PLW[2]"
		INV_REL	"PLW[2]=PLW2"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"f2 channel - power level for pulse (default)"
END
T_NAME		PLdB2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -25.2495 1000
		REL	"if(PLW[2]>0)PLdB2=-10*log(PLW[2])/LN10;else PLdB2=1000;"
		INV_REL	"PLW[2]=0;if(PLdB2<1000)PLW[2]=pow(10.0,(-PLdB2)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power PL2 in dB"
END
T_NAME		PLW12
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"PLW12=PLW[12]"
		INV_REL	"PLW[12]=PLW12"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"f2 channel - power level for CPD/BB decoupling"
END
T_NAME		PLdB12
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -25.2495 1000
		REL	"if(PLW[12]>0)PLdB12=-10*log(PLW[12])/LN10;else PLdB12=1000;"
		INV_REL	"PLW[12]=0;if(PLdB12<1000)PLW[12]=pow(10.0,(-PLdB12)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power PL12 in dB"
END
NAME		SFO2
		FORMAT	"%14.7f MHz"
		TEXT	"frequency of ch. 2"
END
NAME		SPNAM23
TEXT		"jc03_BIBOP.."
END
T_NAME		SPOAL23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL23=SPOAL[23]"
		INV_REL	"SPOAL[23]=SPOAL23"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP23"
END
T_NAME		SPOFFS23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS23=SPOFFS[23]"
		INV_REL	"SPOFFS[23]=SPOFFS23"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP23"
END
T_NAME		SPW23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"SPW23=SPW[23]"
		INV_REL	"SPW[23]=SPW23"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"10 kHz Rf Amplitude"
END
T_NAME		SPdB23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -25.2495 1000
		REL	"if(SPW[23]>0)SPdB23=-10*log(SPW[23])/LN10;elseSPdB23=1000;"
		INV_REL	"SPW[23]=0;if(SPdB23<1000)SPW[23]=pow(10.0,(-SPdB23)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power SPW23 in dB"
END
NAME		SPNAM25
TEXT		"jc05_BEBOP_zy.."
END
T_NAME		SPOAL25
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL25=SPOAL[25]"
		INV_REL	"SPOAL[25]=SPOAL25"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP25"
END
T_NAME		SPOFFS25
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS25=SPOFFS[25]"
		INV_REL	"SPOFFS[25]=SPOFFS25"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP25"
END
T_NAME		SPW25
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"SPW25=SPW[25]"
		INV_REL	"SPW[25]=SPW25"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"10 kHz Rf Amplitude"
END
T_NAME		SPdB25
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -25.2495 1000
		REL	"if(SPW[25]>0)SPdB25=-10*log(SPW[25])/LN10;elseSPdB25=1000;"
		INV_REL	"SPW[25]=0;if(SPdB25<1000)SPW[25]=pow(10.0,(-SPdB25)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power SPW25 in dB"
END
NAME		SPNAM27
TEXT		"jc07_BURBOP_y.."
END
T_NAME		SPOAL27
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL27=SPOAL[27]"
		INV_REL	"SPOAL[27]=SPOAL27"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP27"
END
T_NAME		SPOFFS27
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS27=SPOFFS[27]"
		INV_REL	"SPOFFS[27]=SPOFFS27"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP27"
END
T_NAME		SPW27
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"SPW27=SPW[27]"
		INV_REL	"SPW[27]=SPW27"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"10 kHz Rf Amplitude"
END
T_NAME		SPdB27
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -25.2495 1000
		REL	"if(SPW[27]>0)SPdB27=-10*log(SPW[27])/LN10;elseSPdB27=1000;"
		INV_REL	"SPW[27]=0;if(SPdB27<1000)SPW[27]=pow(10.0,(-SPdB27)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power SPW27 in dB"
END
NAME		SPNAM29
TEXT		"jc09_BEBOP_-yz.."
END
T_NAME		SPOAL29
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL29=SPOAL[29]"
		INV_REL	"SPOAL[29]=SPOAL29"
		FORMAT	"%14.3f"
		TEXT	"phase alignment of freq. offset in SP29"
END
T_NAME		SPOFFS29
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS29=SPOFFS[29]"
		INV_REL	"SPOFFS[29]=SPOFFS29"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"offset frequency for SP29"
END
T_NAME		SPW29
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"SPW29=SPW[29]"
		INV_REL	"SPW[29]=SPW29"
		UNIT	"W"
		FORMAT	"%14.5g W"
TEXT		"10 kHz Rf Amplitude"
END
T_NAME		SPdB29
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -25.2495 1000
		REL	"if(SPW[29]>0)SPdB29=-10*log(SPW[29])/LN10;elseSPdB29=1000;"
		INV_REL	"SPW[29]=0;if(SPdB29<1000)SPW[29]=pow(10.0,(-SPdB29)/10.0)"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power SPW29 in dB"
END
HEADER		"====== GRADIENT CHANNEL ====="
NAME		GPNAM1
TEXT		"SMSQ10.100"
END
NAME		GPNAM2
TEXT		"SMSQ10.100"
END
T_NAME		GPZ1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ1=GPZ[1]"
		INV_REL	"GPZ[1]=GPZ1"
		UNIT	"%"
		FORMAT	"%14.2f %"
TEXT		"80%"
END
T_NAME		GPZ2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ2=GPZ[2]"
		INV_REL	"GPZ[2]=GPZ2"
		UNIT	"%"
		FORMAT	"%14.2f %"
TEXT		"20.1% for C-13, 8.1% for N-15"
END
T_NAME		P16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P16=P[16]"
		INV_REL	"P[16]=P16"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"homospoil/gradient pulse"
END
