EDIT_PAR COMMAND FILE

DI_MODE         LONG
ED_ENTRY        ACQU
ORDER           FILE


HEADER		"F2 - Acquisition Parameters"
T_NAME		Date_
		TYPE	R64
		CLASS	ACQU
		SUBRANGE 0.0 50000000
		REL	"Date_=itodate(DATE)"
		INV_REL	"DATE=datetoi(Date_,DATE)"
		FORMAT	"%14.0f"
		TEXT	" "
END
T_NAME		Time
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"Time=itotime(DATE)"
		INV_REL	"DATE=timetoi(Time,DATE)"
		FORMAT	"%14.2f"
		TEXT	" "
END
NAME		INSTRUM
		TEXT	" "
END
NAME		PROBHD
		FORMAT	"%14.14s"
		TEXT	" "
END
NAME		PULPROG
		TEXT	" "
END
NAME		TD
		TEXT	" "
END
NAME		SOLVENT
		TEXT	" "
END
NAME		NS
		TEXT	" "
END
NAME		DS
		TEXT	" "
END
T_NAME		SWH
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e8
		REL	"SWH=SW*SFO1"
		INV_REL "SW=SWH/SFO1"
		UNIT	"Hz"
		FORMAT	"%14.3f Hz"
		TEXT	" "
END
T_NAME          FIDRES
                TYPE    R32
                CLASS   ACQU
                SUBRANGE 0.0 100000
                REL     "FIDRES=SW*SFO1/TD"
                INV_REL "TD = nextpow(SW*SFO1/FIDRES)"
		UNIT	"Hz"
		FORMAT	"%14.6f Hz"
		TEXT	" "
END
T_NAME          AQ
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000
		REL	"AQ=aqcalc(SW,SFO1,TD,DIGTYP)"
		INV_REL	"TD=tdcalc(SW,SFO1,1.0e6*AQ,DIGTYP)"
		UNIT	"sec"
		FORMAT	"%14.7f sec"
		TEXT	" "
END
NAME		RG
		TEXT	" "
END
T_NAME          DW
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"DW=1/(2*SW*SFO1)"
		INV_REL	"SW=1000000/(2*(0.005+DW)*SFO1)"
		UNIT	"usec"
		FORMAT	"%14.3lf usec"
		TEXT	" "
END
NAME		DE
		FORMAT	"%14.2f usec"
		TEXT	" "
END
NAME		TE
		FORMAT	"%14.1f K"
		TEXT	" "
END
T_NAME		D0
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D0=D[0]"
		INV_REL	"D[0]=D0"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		D1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D1=D[1]"
		INV_REL	"D[1]=D1"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		D5
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D5=D[5]"
		INV_REL	"D[5]=D5"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		D11
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D11=D[11]"
		INV_REL	"D[11]=D11"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		D16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D16=D[16]"
		INV_REL	"D[16]=D16"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		D20
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D20=D[20]"
		INV_REL	"D[20]=D20"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		D21
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D21=D[21]"
		INV_REL	"D[21]=D21"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		D22
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D22=D[22]"
		INV_REL	"D[22]=D22"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		IN0
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"IN0=IN[0]"
		INV_REL	"IN[0]=IN0"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		P1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P1=P[1]"
		INV_REL	"P[1]=P1"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		P2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P2=P[2]"
		INV_REL	"P[2]=P2"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		P3
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P3=P[3]"
		INV_REL	"P[3]=P3"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		P4
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P4=P[4]"
		INV_REL	"P[4]=P4"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
HEADER		"======== CHANNEL f1 ========"
NAME		NUC1
		NONEDIT
		TEXT	" "
END
T_NAME		P21
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P21=P[21]"
		INV_REL	"P[21]=P21"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		P22
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P22=P[22]"
		INV_REL	"P[22]=P22"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		P26
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P26=P[26]"
		INV_REL	"P[26]=P26"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		P30
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P30=P[30]"
		INV_REL	"P[30]=P30"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		PLW1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"PLW1=PLW[1]"
		INV_REL	"PLW[1]=PLW1"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"power PLW1 "
END
NAME		SFO1
		FORMAT	"%14.7f MHz"
		TEXT	" "
END
NAME		SPNAM21
		TEXT	" "
END
T_NAME		SPOAL21
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL21=SPOAL[21]"
		INV_REL	"SPOAL[21]=SPOAL21"
		FORMAT	"%14.3f"
		TEXT	" "
END
T_NAME		SPOFFS21
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS21=SPOFFS[21]"
		INV_REL	"SPOFFS[0]=SPOFFS0"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPW21
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW21=SPW[21]"
		INV_REL	"SPW[21]=SPW21"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"shaped pulse power SPW21"
END
NAME		SPNAM22
		TEXT	" "
END
T_NAME		SPOAL22
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL22=SPOAL[22]"
		INV_REL	"SPOAL[22]=SPOAL22"
		FORMAT	"%14.3f"
		TEXT	" "
END
T_NAME		SPOFFS22
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS22=SPOFFS[22]"
		INV_REL	"SPOFFS[0]=SPOFFS0"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPW22
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW22=SPW[22]"
		INV_REL	"SPW[22]=SPW22"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"shaped pulse power SPW22"
END
NAME		SPNAM24
		TEXT	" "
END
T_NAME		SPOAL24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL24=SPOAL[24]"
		INV_REL	"SPOAL[24]=SPOAL24"
		FORMAT	"%14.3f"
		TEXT	" "
END
T_NAME		SPOFFS24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS24=SPOFFS[24]"
		INV_REL	"SPOFFS[0]=SPOFFS0"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPW24
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW24=SPW[24]"
		INV_REL	"SPW[24]=SPW24"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"shaped pulse power SPW24"
END
NAME		SPNAM26
		TEXT	" "
END
T_NAME		SPOAL26
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL26=SPOAL[26]"
		INV_REL	"SPOAL[26]=SPOAL26"
		FORMAT	"%14.3f"
		TEXT	" "
END
T_NAME		SPOFFS26
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS26=SPOFFS[26]"
		INV_REL	"SPOFFS[0]=SPOFFS0"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPW26
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW26=SPW[26]"
		INV_REL	"SPW[26]=SPW26"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"shaped pulse power SPW26"
END
NAME		SPNAM28
		TEXT	" "
END
T_NAME		SPOAL28
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL28=SPOAL[28]"
		INV_REL	"SPOAL[28]=SPOAL28"
		FORMAT	"%14.3f"
		TEXT	" "
END
T_NAME		SPOFFS28
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS28=SPOFFS[28]"
		INV_REL	"SPOFFS[0]=SPOFFS0"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPW28
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW28=SPW[28]"
		INV_REL	"SPW[28]=SPW28"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"shaped pulse power SPW28"
END
NAME		SPNAM30
		TEXT	" "
END
T_NAME		SPOAL30
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL30=SPOAL[30]"
		INV_REL	"SPOAL[30]=SPOAL30"
		FORMAT	"%14.3f"
		TEXT	" "
END
T_NAME		SPOFFS30
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS30=SPOFFS[30]"
		INV_REL	"SPOFFS[0]=SPOFFS0"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPW30
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW30=SPW[30]"
		INV_REL	"SPW[30]=SPW30"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"shaped pulse power SPW30"
END
NAME		SPNAM31
		TEXT	" "
END
T_NAME		SPOAL31
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL31=SPOAL[31]"
		INV_REL	"SPOAL[31]=SPOAL31"
		FORMAT	"%14.3f"
		TEXT	" "
END
T_NAME		SPOFFS31
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS31=SPOFFS[31]"
		INV_REL	"SPOFFS[0]=SPOFFS0"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPW31
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 86.2469
		REL	"SPW31=SPW[31]"
		INV_REL	"SPW[31]=SPW31"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"shaped pulse power SPW31"
END
HEADER		"======== CHANNEL f2 ========"
NAME		NUC2
		NONEDIT
		TEXT	" "
END
T_NAME		P27
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P27=P[27]"
		INV_REL	"P[27]=P27"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		PLW2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"PLW2=PLW[2]"
		INV_REL	"PLW[2]=PLW2"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"power PLW2 "
END
T_NAME		PLW12
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"PLW12=PLW[12]"
		INV_REL	"PLW[12]=PLW12"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"power PLW12 "
END
NAME		SFO2
		FORMAT	"%14.7f MHz"
		TEXT	" "
END
NAME		SPNAM23
		TEXT	" "
END
T_NAME		SPOAL23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL23=SPOAL[23]"
		INV_REL	"SPOAL[23]=SPOAL23"
		FORMAT	"%14.3f"
		TEXT	" "
END
T_NAME		SPOFFS23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS23=SPOFFS[23]"
		INV_REL	"SPOFFS[0]=SPOFFS0"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPW23
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"SPW23=SPW[23]"
		INV_REL	"SPW[23]=SPW23"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"shaped pulse power SPW23"
END
NAME		SPNAM25
		TEXT	" "
END
T_NAME		SPOAL25
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL25=SPOAL[25]"
		INV_REL	"SPOAL[25]=SPOAL25"
		FORMAT	"%14.3f"
		TEXT	" "
END
T_NAME		SPOFFS25
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS25=SPOFFS[25]"
		INV_REL	"SPOFFS[0]=SPOFFS0"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPW25
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"SPW25=SPW[25]"
		INV_REL	"SPW[25]=SPW25"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"shaped pulse power SPW25"
END
NAME		SPNAM27
		TEXT	" "
END
T_NAME		SPOAL27
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL27=SPOAL[27]"
		INV_REL	"SPOAL[27]=SPOAL27"
		FORMAT	"%14.3f"
		TEXT	" "
END
T_NAME		SPOFFS27
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS27=SPOFFS[27]"
		INV_REL	"SPOFFS[0]=SPOFFS0"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPW27
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"SPW27=SPW[27]"
		INV_REL	"SPW[27]=SPW27"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"shaped pulse power SPW27"
END
NAME		SPNAM29
		TEXT	" "
END
T_NAME		SPOAL29
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1.0 1.0
		REL	"SPOAL29=SPOAL[29]"
		INV_REL	"SPOAL[29]=SPOAL29"
		FORMAT	"%14.3f"
		TEXT	" "
END
T_NAME		SPOFFS29
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"SPOFFS29=SPOFFS[29]"
		INV_REL	"SPOFFS[0]=SPOFFS0"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPW29
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 327.3
		REL	"SPW29=SPW[29]"
		INV_REL	"SPW[29]=SPW29"
		UNIT	"W"
		FORMAT	"%14.8f W"
		TEXT	"shaped pulse power SPW29"
END
HEADER		"====== GRADIENT CHANNEL ====="
NAME		GPNAM1
		TEXT	" "
END
NAME		GPNAM2
		TEXT	" "
END
T_NAME		GPZ1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ1=GPZ[1]"
		INV_REL	"GPZ[1]=GPZ1"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ2=GPZ[2]"
		INV_REL	"GPZ[2]=GPZ2"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		P16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P16=P[16]"
		INV_REL	"P[16]=P16"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
